("FILE_TYPE"	"PMAP File"
    ("devices"
        ("VDC")
        ("R")
        ("L")
        ("diode")
        ("CM300DY-24H")
        ("VPULSE")
        ("Param")
    )
    ("instances"
        ("Vd1"
            ("device_name"	"VDC")
            ("pspice_path"	"V_Vd1")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"150V")
                    ("pspice_param"	"DC")
                )
                ("BiasValue Power"
                    ("value"	"-76.05mW")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("R1"
            ("device_name"	"R")
            ("pspice_path"	"R_R1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"{Rload}")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"4.900W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("L1"
            ("device_name"	"L")
            ("pspice_path"	"L_L1")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"{Lload}")
                    ("pspice_param"	"VALUE")
                )
                ("IC"
                    ("value"	"-7A")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"-8.942W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("CURRENT"
                    ("value"	"LMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("DIELECTRIC"
                    ("value"	"DSMAX")
                    ("pspice_param"	"DIELECTRIC")
                )
            )
        )
        ("L2"
            ("device_name"	"L")
            ("pspice_path"	"L_L2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"{Lload}")
                    ("pspice_param"	"VALUE")
                )
                ("IC"
                    ("value"	"-7A")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"-8.942W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("CURRENT"
                    ("value"	"LMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("DIELECTRIC"
                    ("value"	"DSMAX")
                    ("pspice_param"	"DIELECTRIC")
                )
            )
        )
        ("R2"
            ("device_name"	"R")
            ("pspice_path"	"R_R2")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"{Rload}")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"4.900W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("L3"
            ("device_name"	"L")
            ("pspice_path"	"L_L3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"{Lload}")
                    ("pspice_param"	"VALUE")
                )
                ("IC"
                    ("value"	"14A")
                    ("pspice_param"	"IC")
                )
                ("BiasValue Power"
                    ("value"	"-35.77W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("CURRENT"
                    ("value"	"LMAX")
                    ("pspice_param"	"CURRENT")
                )
                ("DIELECTRIC"
                    ("value"	"DSMAX")
                    ("pspice_param"	"DIELECTRIC")
                )
            )
        )
        ("R3"
            ("device_name"	"R")
            ("pspice_path"	"R_R3")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"{Rload}")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"19.60W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
            )
        )
        ("Rgc-"
            ("device_name"	"R")
            ("pspice_path"	"R_Rgc-")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("Dc-"
            ("device_name"	"diode")
            ("pspice_path"	"d_Dc-")
            ("level"	"0")
            ("model_params"
                ("RS"
                    ("value"	"1m")
                    ("pspice_param"	"AREA")
                )
                ("BiasValue Power"
                    ("value"	"12.82W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("Schematics' Source Library"
                    ("value"	"C:\\Dokument\\Kraftelektronik 1 - 2009\\PSpice Exercise 1\\Libraries\\pspice9\\pwr_elec.slb")
                    ("pspice_param"	"Schematics' Source Library")
                )
            )
        )
        ("Tc-"
            ("device_name"	"CM300DY-24H")
            ("pspice_path"	"Z_Tc-")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"6.637nW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("COMPONENT"
                    ("value"	"CM300DY-24H")
                    ("pspice_param"	"COMPONENT")
                )
            )
        )
        ("Rgc+"
            ("device_name"	"R")
            ("pspice_path"	"R_Rgc+")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("Tc+"
            ("device_name"	"CM300DY-24H")
            ("pspice_path"	"Z_Tc+")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"51.00mW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("COMPONENT"
                    ("value"	"CM300DY-24H")
                    ("pspice_param"	"COMPONENT")
                )
            )
        )
        ("Dc+"
            ("device_name"	"diode")
            ("pspice_path"	"d_Dc+")
            ("level"	"0")
            ("model_params"
                ("RS"
                    ("value"	"1m")
                    ("pspice_param"	"AREA")
                )
                ("BiasValue Power"
                    ("value"	"90.55nW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("Schematics' Source Library"
                    ("value"	"C:\\Dokument\\Kraftelektronik 1 - 2009\\PSpice Exercise 1\\Libraries\\pspice9\\pwr_elec.slb")
                    ("pspice_param"	"Schematics' Source Library")
                )
            )
        )
        ("Db+"
            ("device_name"	"diode")
            ("pspice_path"	"d_Db+")
            ("level"	"0")
            ("model_params"
                ("RS"
                    ("value"	"1m")
                    ("pspice_param"	"AREA")
                )
                ("BiasValue Power"
                    ("value"	"89.51nW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("Schematics' Source Library"
                    ("value"	"C:\\Dokument\\Kraftelektronik 1 - 2009\\PSpice Exercise 1\\Libraries\\pspice9\\pwr_elec.slb")
                    ("pspice_param"	"Schematics' Source Library")
                )
            )
        )
        ("Tb+"
            ("device_name"	"CM300DY-24H")
            ("pspice_path"	"Z_Tb+")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"50.53mW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("COMPONENT"
                    ("value"	"CM300DY-24H")
                    ("pspice_param"	"COMPONENT")
                )
            )
        )
        ("Rgb+"
            ("device_name"	"R")
            ("pspice_path"	"R_Rgb+")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("Rgb-"
            ("device_name"	"R")
            ("pspice_path"	"R_Rgb-")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("Tb-"
            ("device_name"	"CM300DY-24H")
            ("pspice_path"	"Z_Tb-")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"5.341W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("COMPONENT"
                    ("value"	"CM300DY-24H")
                    ("pspice_param"	"COMPONENT")
                )
            )
        )
        ("Db-"
            ("device_name"	"diode")
            ("pspice_path"	"d_Db-")
            ("level"	"0")
            ("model_params"
                ("RS"
                    ("value"	"1m")
                    ("pspice_param"	"AREA")
                )
                ("BiasValue Power"
                    ("value"	"674.6fW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("Schematics' Source Library"
                    ("value"	"C:\\Dokument\\Kraftelektronik 1 - 2009\\PSpice Exercise 1\\Libraries\\pspice9\\pwr_elec.slb")
                    ("pspice_param"	"Schematics' Source Library")
                )
            )
        )
        ("Rga-"
            ("device_name"	"R")
            ("pspice_path"	"R_Rga-")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"1.570e-21W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("Ta-"
            ("device_name"	"CM300DY-24H")
            ("pspice_path"	"Z_Ta-")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"5.364W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("COMPONENT"
                    ("value"	"CM300DY-24H")
                    ("pspice_param"	"COMPONENT")
                )
            )
        )
        ("Da-"
            ("device_name"	"diode")
            ("pspice_path"	"d_Da-")
            ("level"	"0")
            ("model_params"
                ("RS"
                    ("value"	"1m")
                    ("pspice_param"	"AREA")
                )
                ("BiasValue Power"
                    ("value"	"674.6fW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("Schematics' Source Library"
                    ("value"	"C:\\Dokument\\Kraftelektronik 1 - 2009\\PSpice Exercise 1\\Libraries\\pspice9\\pwr_elec.slb")
                    ("pspice_param"	"Schematics' Source Library")
                )
            )
        )
        ("Da+"
            ("device_name"	"diode")
            ("pspice_path"	"d_Da+")
            ("level"	"0")
            ("model_params"
                ("RS"
                    ("value"	"1m")
                    ("pspice_param"	"AREA")
                )
                ("BiasValue Power"
                    ("value"	"89.51nW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("Schematics' Source Library"
                    ("value"	"C:\\Dokument\\Kraftelektronik 1 - 2009\\PSpice Exercise 1\\Libraries\\pspice9\\pwr_elec.slb")
                    ("pspice_param"	"Schematics' Source Library")
                )
            )
        )
        ("Rga+"
            ("device_name"	"R")
            ("pspice_path"	"R_Rga+")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"155.1e-27W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("Ta+"
            ("device_name"	"CM300DY-24H")
            ("pspice_path"	"Z_Ta+")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"50.53mW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("COMPONENT"
                    ("value"	"CM300DY-24H")
                    ("pspice_param"	"COMPONENT")
                )
            )
        )
        ("Va+"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_Va+")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"-271.4e-27W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PER"
                    ("value"	"{1/freq}")
                    ("pspice_param"	"PER")
                )
                ("TF"
                    ("value"	"200n")
                    ("pspice_param"	"TF")
                )
                ("TR"
                    ("value"	"200n")
                    ("pspice_param"	"TR")
                )
                ("V2"
                    ("value"	"15")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("TD"
                    ("value"	"200n")
                    ("pspice_param"	"TD")
                )
                ("PW"
                    ("value"	"{0.5/freq}")
                    ("pspice_param"	"PW")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
            )
        )
        ("Va-"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_Va-")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"594.4pW")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PW"
                    ("value"	"{{0.5/freq}+400n}")
                    ("pspice_param"	"PW")
                )
                ("TD"
                    ("value"	"0")
                    ("pspice_param"	"TD")
                )
                ("V1"
                    ("value"	"15")
                    ("pspice_param"	"V1")
                )
                ("V2"
                    ("value"	"0")
                    ("pspice_param"	"V2")
                )
                ("TR"
                    ("value"	"200n")
                    ("pspice_param"	"TR")
                )
                ("TF"
                    ("value"	"200n")
                    ("pspice_param"	"TF")
                )
                ("PER"
                    ("value"	"{1/freq}")
                    ("pspice_param"	"PER")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
            )
        )
        ("Vb+"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_Vb+")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PER"
                    ("value"	"{1/freq}")
                    ("pspice_param"	"PER")
                )
                ("TF"
                    ("value"	"200n")
                    ("pspice_param"	"TF")
                )
                ("TR"
                    ("value"	"200n")
                    ("pspice_param"	"TR")
                )
                ("V2"
                    ("value"	"15")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("TD"
                    ("value"	"{1/(3*freq)+200n}")
                    ("pspice_param"	"TD")
                )
                ("PW"
                    ("value"	"{0.5/freq}")
                    ("pspice_param"	"PW")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
            )
        )
        ("Vc+"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_Vc+")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PER"
                    ("value"	"{1/freq}")
                    ("pspice_param"	"PER")
                )
                ("TF"
                    ("value"	"200n")
                    ("pspice_param"	"TF")
                )
                ("TR"
                    ("value"	"200n")
                    ("pspice_param"	"TR")
                )
                ("V2"
                    ("value"	"15")
                    ("pspice_param"	"V2")
                )
                ("V1"
                    ("value"	"0")
                    ("pspice_param"	"V1")
                )
                ("TD"
                    ("value"	"{2/(3*freq)+200n}")
                    ("pspice_param"	"TD")
                )
                ("PW"
                    ("value"	"{0.5/freq}")
                    ("pspice_param"	"PW")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
            )
        )
        ("Vb-"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_Vb-")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PW"
                    ("value"	"{{0.5/freq}+400n}")
                    ("pspice_param"	"PW")
                )
                ("TD"
                    ("value"	"{1/(3*freq)}")
                    ("pspice_param"	"TD")
                )
                ("V1"
                    ("value"	"15")
                    ("pspice_param"	"V1")
                )
                ("V2"
                    ("value"	"0")
                    ("pspice_param"	"V2")
                )
                ("TR"
                    ("value"	"200n")
                    ("pspice_param"	"TR")
                )
                ("TF"
                    ("value"	"200n")
                    ("pspice_param"	"TF")
                )
                ("PER"
                    ("value"	"{1/freq}")
                    ("pspice_param"	"PER")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
            )
        )
        ("Vc-"
            ("device_name"	"VPULSE")
            ("pspice_path"	"V_Vc-")
            ("level"	"0")
            ("model_params"
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("PW"
                    ("value"	"{{0.5/freq}+400n}")
                    ("pspice_param"	"PW")
                )
                ("TD"
                    ("value"	"{2/(3*freq)}")
                    ("pspice_param"	"TD")
                )
                ("V1"
                    ("value"	"15")
                    ("pspice_param"	"V1")
                )
                ("V2"
                    ("value"	"0")
                    ("pspice_param"	"V2")
                )
                ("TR"
                    ("value"	"200n")
                    ("pspice_param"	"TR")
                )
                ("TF"
                    ("value"	"200n")
                    ("pspice_param"	"TF")
                )
                ("PER"
                    ("value"	"{1/freq}")
                    ("pspice_param"	"PER")
                )
                ("DC"
                    ("value"	"")
                    ("pspice_param"	"DC")
                )
                ("AC"
                    ("value"	"")
                    ("pspice_param"	"AC")
                )
            )
        )
        ("Vd2"
            ("device_name"	"VDC")
            ("pspice_path"	"V_Vd2")
            ("level"	"0")
            ("model_params"
                ("DC"
                    ("value"	"150V")
                    ("pspice_param"	"DC")
                )
                ("BiasValue Power"
                    ("value"	"-76.05mW")
                    ("pspice_param"	"BiasValue Power")
                )
            )
        )
        ("R5"
            ("device_name"	"R")
            ("pspice_path"	"R_R5")
            ("level"	"0")
            ("model_params"
                ("VALUE"
                    ("value"	"1m")
                    ("pspice_param"	"VALUE")
                )
                ("BiasValue Power"
                    ("value"	"0W")
                    ("pspice_param"	"BiasValue Power")
                )
                ("DIST"
                    ("value"	"FLAT")
                    ("pspice_param"	"DIST")
                )
                ("TOLERANCE"
                    ("value"	"")
                    ("pspice_param"	"TOLERANCE")
                )
                ("VOLTAGE"
                    ("value"	"RVMAX")
                    ("pspice_param"	"VOLTAGE")
                )
                ("SLOPE"
                    ("value"	"RSMAX")
                    ("pspice_param"	"SLOPE")
                )
                ("MAX_TEMP"
                    ("value"	"RTMAX")
                    ("pspice_param"	"MAX_TEMP")
                )
                ("POWER"
                    ("value"	"RMAX")
                    ("pspice_param"	"POWER")
                )
                ("TC1"
                    ("value"	"0")
                    ("pspice_param"	"TC1")
                )
                ("TC2"
                    ("value"	"0")
                    ("pspice_param"	"TC2")
                )
            )
        )
        ("PARAM"
            ("device_name"	"Param")
            ("pspice_path"	"")
            ("level"	"0")
            ("model_params"
                ("rload"
                    ("value"	"1")
                    ("pspice_param"	"rload")
                )
                ("freq"
                    ("value"	"50hz")
                    ("pspice_param"	"freq")
                )
                ("lload"
                    ("value"	"10u")
                    ("pspice_param"	"lload")
                )
            )
        )
    )
)
