
hpeesofsim (*) 470.shp Oct 20 2017, MINT version 4
    (64-bit linux built: Sat Oct 21, 2017 04:03:36 +0000)
Copyright 1989 - 2017 Keysight Technologies.

Warning detected by hpeesofsim in Substrate model during netlist flattening.
    Simulations referencing substrate `MSub1' will not include metal loss
    because metal thickness is zero.

CT Sweep1[1] <LET564_CROFT_lib:stubbanpassning:schematic>   L=(0->20)

SP Sweep1[1].SP1[1/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=0  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[2/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=500e-03  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[3/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=1  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[4/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=1.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[5/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=2  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[6/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=2.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[7/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=3  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[8/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=3.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[9/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=4  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[10/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=4.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[11/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[12/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=5.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[13/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=6  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[14/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=6.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[15/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=7  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[16/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=7.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[17/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=8  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[18/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=8.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[19/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=9  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[20/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=9.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[21/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=10  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[22/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=10.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[23/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=11  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[24/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=11.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[25/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=12  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[26/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=12.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[27/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=13  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[28/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=13.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[29/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=14  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[30/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=14.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[31/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=15  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[32/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=15.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[33/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=16  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[34/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=16.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[35/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=17  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[36/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=17.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[37/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=18  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[38/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=18.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[39/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=19  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[40/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=19.5  freq=(0 Hz->2 GHz)


SP Sweep1[1].SP1[41/41] <LET564_CROFT_lib:stubbanpassning:schematic>  L=20  freq=(0 Hz->2 GHz)


Resource usage:
    User time                 =     1.88 seconds.
    System time               =     0.63 seconds.
    Total CPU time            =     2.51 seconds.
    Simulation stopwatch time =     1.00 seconds.
    Total stopwatch time      =     2.81 seconds.

    Physical memory used: 73.6 MBytes.
    Incremental virtual memory (data only) used:  27.1 MBytes.

