
hpeesofsim (*) 450.shp Jan 21 2016, MINT version 4
    (64-bit linux built: 01/21/16 15:12:01)
Copyright 1995 - 2015 Keysight Technologies, 1989-2016.

Pt DC convergence is used.
Warning detected by hpeesofsim during DC analysis `SP2'.
    Circuit converged after a virtual resistance of 1 TOhms 
    was added between each node and ground, and a virtual 
    resistance of 1 pOhms was inserted in each current branch. 
    Possible causes include floating nodes or missing ground.

SP SP2[1] <LET564_CROFT_lib:amplifier_layout_test:schematic>   freq=(1 GHz->3 GHz)
Warning detected by hpeesofsim during SP analysis `SP2'.
    The simulation temperature (25.0 C) is not the same as the IEEE standard
    noise temperature (290 K or 16.85 C) in the noise analysis `SP2'.
    If the simulation temperature is not equal to the IEEE standard temperature,
    then the loss and the noise figure will not agree for a passive circuit.
    The `Temp' parameter on the Options item can be set to 16.85 C to
    eliminate this warning message.

,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,

Resource usage:
    User time                 =     4.07 seconds.
    System time               =     0.49 seconds.
    Total CPU time            =     4.56 seconds.
    Simulation stopwatch time =     3.91 seconds.
    Total stopwatch time      =     4.86 seconds.

    Physical memory used: 77.3 MBytes.
    Incremental virtual memory (data only) used:  33.9 MBytes.

