
hpeesofsim (*) 470.shp Oct 20 2017, MINT version 4
    (64-bit linux built: Sat Oct 21, 2017 04:03:36 +0000)
Copyright 1989 - 2017 Keysight Technologies.

Pt DC convergence is used.

SP SP1[1] <LET564_CROFT_lib:stabiliseringsnat:schematic>   freq=2.01 GHz
Warning detected by hpeesofsim during SP analysis `SP1'.
    The simulation temperature (25.0 C) is not the same as the IEEE standard
    noise temperature (290 K or 16.85 C) in the noise analysis `SP1'.
    If the simulation temperature is not equal to the IEEE standard temperature,
    then the loss and the noise figure will not agree for a passive circuit.
    The `Temp' parameter on the Options item can be set to 16.85 C to
    eliminate this warning message.



Resource usage:
    User time                 =     2.11 seconds.
    System time               =     1.09 seconds.
    Total CPU time            =     3.20 seconds.
    Simulation stopwatch time =     0.52 seconds.
    Total stopwatch time      =     2.25 seconds.

    Physical memory used: 75 MBytes.
    Incremental virtual memory (data only) used:  24.9 MBytes.

