<?xml version="1.0" encoding="UTF-8"?>
<spirit:design xmlns:xilinx="http://www.xilinx.com" xmlns:spirit="http://www.spiritconsortium.org/XMLSchema/SPIRIT/1685-2009" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
  <spirit:vendor>xilinx.com</spirit:vendor>
  <spirit:library>xci</spirit:library>
  <spirit:name>unknown</spirit:name>
  <spirit:version>1.0</spirit:version>
  <spirit:componentInstances>
    <spirit:componentInstance>
      <spirit:instanceName>pdm_to_pcm_cic_compiler_0_0</spirit:instanceName>
      <spirit:componentRef spirit:vendor="xilinx.com" spirit:library="ip" spirit:name="cic_compiler" spirit:version="4.0"/>
      <spirit:configurableElementValues>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLKEN_INTF.POLARITY">ACTIVE_LOW</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.CLK_DOMAIN">/clk_wiz_0_clk_out1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.FREQ_HZ">18431963</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.PHASE">0.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.ARESETN_INTF.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.EVENT_HALTED_INTF.PortWidth">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.EVENT_TLAST_MISSING_INTF.PortWidth">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.EVENT_TLAST_UNEXPECTED_INTF.PortWidth">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.CLK_DOMAIN">/clk_wiz_0_clk_out1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.FREQ_HZ">18431963</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.HAS_TKEEP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.HAS_TLAST">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.HAS_TREADY">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.HAS_TSTRB">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.LAYERED_METADATA">xilinx.com:interface:datatypes:1.0 {TDATA {datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type automatic dependency {} format long minimum {} maximum {}} value 94} bitoffset {attribs {resolve_type immediate dependency {} format long minimum {} maximum {}} value 0} array_type {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value chan} size {attribs {resolve_type gener
ated dependency chan_size format long minimum {} maximum {}} value 4} stride {attribs {resolve_type generated dependency chan_stride format long minimum {} maximum {}} value 24} datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type generated dependency data_width format long minimum {} maximum {}} value 22} bitoffset {attribs {resolve_type immediate dependency {} format long minimum {} maximum {}} value 0} rea
l {fixed {fractwidth {attribs {resolve_type generated dependency data_fractwidth format long minimum {} maximum {}} value 0} signed {attribs {resolve_type immediate dependency {} format bool minimum {} maximum {}} value true}}}}}}} TDATA_WIDTH 24 TUSER {datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type automatic dependency {} format long minimum {} maximum {}} value 9} bitoffset {attribs {resolve_type imme
diate dependency {} format long minimum {} maximum {}} value 0} struct {field_chan_out {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value chan_out} enabled {attribs {resolve_type generated dependency enabled format bool minimum {} maximum {}} value true} datatype {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type generated dependency chan_out_width format long minimum {} 
maximum {}} value 2} bitoffset {attribs {resolve_type immediate dependency {} format long minimum {} maximum {}} value 0} integer {signed {attribs {resolve_type immediate dependency {} format bool minimum {} maximum {}} value false}}}} field_chan_sync {name {attribs {resolve_type immediate dependency {} format string minimum {} maximum {}} value chan_sync} enabled {attribs {resolve_type generated dependency enabled format bool minimum {} maximum {}} value true} datatype {name {attribs {resolve_t
ype immediate dependency {} format string minimum {} maximum {}} value {}} bitwidth {attribs {resolve_type generated dependency chan_sync_width format long minimum {} maximum {}} value 1} bitoffset {attribs {resolve_type generated dependency chan_sync_offset format long minimum {} maximum {}} value 8}}}}}} TUSER_WIDTH 16}</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.PHASE">0.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.TDATA_NUM_BYTES">3</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.TDEST_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.TID_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.TUSER_WIDTH">16</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.CLK_DOMAIN"/>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.FREQ_HZ">100000000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.HAS_TKEEP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.HAS_TLAST">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.HAS_TREADY">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.HAS_TSTRB">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.LAYERED_METADATA">undef</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.PHASE">0.000</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.TDATA_NUM_BYTES">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.TDEST_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.TID_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_CONFIG.TUSER_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.CLK_DOMAIN">/clk_wiz_0_clk_out1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.FREQ_HZ">18431963</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.HAS_TKEEP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.HAS_TLAST">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.HAS_TREADY">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.HAS_TSTRB">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.INSERT_VIP">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.LAYERED_METADATA">undef</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.PHASE">0.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.TDATA_NUM_BYTES">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.TDEST_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.TID_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.TUSER_WIDTH">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_C1">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_C2">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_C3">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_C4">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_C5">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_C6">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_CLK_FREQ">4</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_COMPONENT_NAME">pdm_to_pcm_cic_compiler_0_0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_DIFF_DELAY">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_FAMILY">artix7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_FILTER_TYPE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_ACLKEN">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_ARESETN">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_DOUT_TREADY">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_HAS_ROUNDING">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_I1">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_I2">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_I3">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_I4">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_I5">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_I6">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_INPUT_WIDTH">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_MAX_RATE">16</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_MIN_RATE">16</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_M_AXIS_DATA_TDATA_WIDTH">24</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_M_AXIS_DATA_TUSER_WIDTH">16</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_NUM_CHANNELS">4</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_NUM_STAGES">5</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_OUTPUT_WIDTH">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_RATE">16</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_RATE_TYPE">0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_SAMPLE_FREQ">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_S_AXIS_CONFIG_TDATA_WIDTH">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_S_AXIS_DATA_TDATA_WIDTH">8</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_USE_DSP">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_USE_STREAMING_INTERFACE">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="MODELPARAM_VALUE.C_XDEVICEFAMILY">artix7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Clock_Frequency">12.8</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Component_Name">pdm_to_pcm_cic_compiler_0_0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Differential_Delay">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Filter_Type">Decimation</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Fixed_Or_Initial_Rate">16</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.GUI_Behaviour">Coregen</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.HAS_ACLKEN">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.HAS_ARESETN">false</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.HAS_DOUT_TREADY">true</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.HardwareOversamplingRate">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Input_Data_Width">2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Input_Sample_Frequency">3.2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Maximum_Rate">16</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Minimum_Rate">16</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Number_Of_Channels">4</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Number_Of_Stages">5</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Output_Data_Width">22</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Passband_Max">0.5</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Passband_Min">0.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Quantization">Full_Precision</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.RateSpecification">Frequency_Specification</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Response_Magnitude">Normalized</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.SamplePeriod">1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Sample_Rate_Changes">Fixed</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Stopband_Max">1.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Stopband_Min">0.5</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Use_Streaming_Interface">true</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PARAM_VALUE.Use_Xtreme_DSP_Slice">true</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.ARCHITECTURE">artix7</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.BASE_BOARD_PART">xilinx.com:ac701:part0:1.0</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.BOARD_CONNECTIONS"/>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.DEVICE">xc7a200t</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.PACKAGE">fbg676</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.PREFHDL">VHDL</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.SILICON_REVISION"/>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.SIMULATOR_LANGUAGE">MIXED</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.SPEEDGRADE">-2</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.STATIC_POWER"/>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.TEMPERATURE_GRADE"/>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.USE_RDI_CUSTOMIZATION">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="PROJECT_PARAM.USE_RDI_GENERATION">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.IPCONTEXT">IP_Integrator</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.IPREVISION">14</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.MANAGED">TRUE</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.OUTPUTDIR">.</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SELECTEDSIMMODEL"/>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SHAREDDIR">../../ipshared</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SWVERSION">2019.1</spirit:configurableElementValue>
        <spirit:configurableElementValue spirit:referenceId="RUNTIME_PARAM.SYNTHESISFLOW">OUT_OF_CONTEXT</spirit:configurableElementValue>
      </spirit:configurableElementValues>
      <spirit:vendorExtensions>
        <xilinx:componentInstanceExtensions>
          <xilinx:configElementInfos>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.CLK_DOMAIN" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.FREQ_HZ" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.ACLK_INTF.PHASE" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.CLK_DOMAIN" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.FREQ_HZ" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.HAS_TKEEP" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.HAS_TLAST" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.HAS_TREADY" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.HAS_TSTRB" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.LAYERED_METADATA" xilinx:valueSource="user" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.PHASE" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.TDATA_NUM_BYTES" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.TDEST_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.TID_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.M_AXIS_DATA.TUSER_WIDTH" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.CLK_DOMAIN" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.FREQ_HZ" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.HAS_TKEEP" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.HAS_TLAST" xilinx:valueSource="auto" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.HAS_TREADY" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.HAS_TSTRB" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.PHASE" xilinx:valueSource="ip_propagated" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.TDATA_NUM_BYTES" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.TDEST_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.TID_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="BUSIFPARAM_VALUE.S_AXIS_DATA.TUSER_WIDTH" xilinx:valueSource="constant" xilinx:valuePermission="bd"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Clock_Frequency" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Filter_Type" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Fixed_Or_Initial_Rate" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.HAS_DOUT_TREADY" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Input_Data_Width" xilinx:valueSource="user" xilinx:valuePermission="bd_and_user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Input_Sample_Frequency" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Maximum_Rate" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Minimum_Rate" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Number_Of_Channels" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Number_Of_Stages" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.Output_Data_Width" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.RateSpecification" xilinx:valueSource="user"/>
            <xilinx:configElementInfo xilinx:referenceId="PARAM_VALUE.SamplePeriod" xilinx:valueSource="user"/>
          </xilinx:configElementInfos>
        </xilinx:componentInstanceExtensions>
      </spirit:vendorExtensions>
    </spirit:componentInstance>
  </spirit:componentInstances>
</spirit:design>
